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	Product Description
	A new generation, water based 100% acrylic, long-life, interior / exterior, high gloss coating.

	Application Areas
	· Interior and exterior use.

· High traffic areas that need a highly washable and durable coating in a wide range of colours.

· Primed plaster, hardboard and fibre cement walls.

· Primed metal and wooden substrates.

· Adheres to difficult substrates such as chipboard, concrete, baked enamel coatings and galvanised metal.

· Ideal coating for gutters and down pipes where no primer is required.

· In humid coastal areas Dynamiq Waterbased Enamel Paint is ideal for recoating exterior wood finishes. Due to its good water permeability no blistering will take place.

	Product Features
	· Highly durable and UV resistant.

· Highly washable, cleanable.

· Excellent adhesion to a range of properly prepared substrates.

· High hiding power and film build.

· Dries to a hard-wearing gloss finish for interior and exterior use.

· Has outstanding resistance against humidity, alkaline attack, UV light and has excellent gloss retention. This makes Dynamiq Waterbased Enamel Paint a viable alternative to solvent-based high gloss enamel paint.

· More humidity, chemical and UV light resistant than standard high-gloss enamel paint.

· Two coats of Dynamiq Waterbased Enamel Paint are applied for best results.

	Product Data
	Resin Base
	Pure acrylic resin emulsion

	
	Drying Time
	Touch dry: 1-2 hour

Hard dry: ± 4-6 hours

(In Humid or Cold Weather up to 2 hours touch dry and 6-8 hours hard dry)

	
	Film Thickness
	30 – 40 microns Per Coat

	
	Spreading Rate
	Approximately 10 square metres per litre.

Although the spreading rate will vary with porosity and type of substrate, for uncoated new surfaces work on 8-10 square metres per litre for the first coat and 10-12 square metres per litre for subsequent coats and when applied to sealed, previously painted substrates.

	
	Surface Appearance
	Gloss finish

	
	Density
	Depending on colour

	Application Details
	

	· Mixing
	Always stir well before use with a flat paddle.

	· Application Method
	Brush, roller or airless spray (high-pressure air spray is not recommended).

	· Thinning
	Dynamiq Waterbased Enamel Paint is ready for use un-thinned; thinning with water will reduce its hiding power.

	· Cleaning
	Water.

	· Application
	· Stir well before use.

· Two coats of Dynamiq Waterbased Enamel Paint are applied for best results.

· With brush or roller, apply a generous coat of Dynamiq  Waterbased Enamel Paint (airless NOT high-pressure spray can be used for large areas if required).

· Allow to dry overnight before recoating.

· Apply a second generous coat of Dynamiq Waterbased Enamel Paint.
· Clean up application equipment with water. Clean tools immediately after use - once dry, this paint does not dissolve in water.

· Do not apply before 09:00 and after 16:00 in the winter.

· Although the spreading rate will vary with porosity and type of substrate, for uncoated new surfaces work on 8-10 square metres per litre for the first coat and 10-12 square metres per litre for subsequent coats and when applied to sealed, previously painted substrates.

· Do not apply exterior if it looks like rain will occur within 4-6 hours of application.

	Surface Preparation
	

	· Mild Steel

          (Renovation)
	· Affected areas need to be cleaned back to bright metal and spot primed with a water based metal primer.

· Sand existing coating.

· With brush or roller, apply a generous coat of Dynamiq Waterbased Enamel Paint (airless NOT high-pressure spray can be used for large areas if required).

· Allow to dry overnight before recoating.

· Apply a second generous coat of Dynamiq Waterbased Enamel Paint.

	· Mild Steel 

          (New)
	· Degrease surfaces to remove the manufacturer’s grease protective layer. This process is repeated until the surface is water break free.

· After drying, the whole substrate is coated with WB Metal Primer (it is absolutely essential to firstly apply one coat of WB Metal Primer.  Acrylic based paints should never come into direct contact with mild steel).

· With brush or roller, apply a generous coat of Dynamiq Waterbased Enamel Paint (airless NOT high-pressure spray can be used for large areas if required).

· Allow to dry overnight before recoating.

· Apply a second generous coat of Dynamiq Waterbased Enamel Paint.

	· Uncoated Concrete Surfaces

· Raw / New Plaster

· Precast
	· Make sure surface is dry and firm.

· Remove all dust, foreign material, fungal and algae growth.

· Fill and seal all visible cracks with a suitable crack filler.
· Apply one coat of Dynamiq Bonding Liquid to cover the crack filler
· Sand well and remove dust.

· Prime with Dynamiq Plaster Primer.

· With brush or roller, apply a generous coat of Dynamiq Waterbased Enamel Paint (airless NOT high-pressure spray can be used for large areas if required).

· Allow to dry overnight before recoating.

· Apply a second generous coat of Dynamiq Waterbased Enamel Paint.


	· Uncoated, Weathered or New Fibre Cement Surfaces
	· Remove dust, foreign material, fungal and algae growth.

· If friable or powdery, seal with Dynamiq Bonding Liquid.

· With brush or roller, apply a generous coat of Dynamiq Waterbased Enamel Paint  (airless NOT high-pressure spray can be used for large areas if required).

· Allow to dry overnight before recoating.

· Apply a second generous coat of Dynamiq Waterbased Enamel Paint.

	· Previously Painted Surfaces

· Precast
	· Surface must be in a sound condition.

· Existing gloss finishes should be well sanded.

· Remove all loose, flaking and bubbling paint.

· Remove all dust, foreign material, fungal and algae growth.

· Allow to dry.

· Fill and seal all visible cracks with a suitable crack filler.

· Apply one coat of Dynamiq Bonding Liquid to seal the crack filler
· With brush or roller, apply a generous coat of Dynamiq Waterbased Enamel Paint (airless NOT high pressure spray can be used for large areas if required).

· Allow to dry overnight before recoating.

· Apply a second generous coat of Dynamiq Waterbased Enamel Paint.

	· Wooden Surfaces and Chipboard
	· Use wood filler for filling holes, cracks and unevenness on wood.

· Apply one coat of Dynamiq Bonding liquid to cover the wood filler. 
· For exterior use a wood primer is recommended.

· With brush or roller, apply a generous coat of Dynamiq Waterbased Enamel Paint (airless NOT high- pressure spray can be used for large areas if required).

· Allow to dry overnight before recoating.

· Apply a second generous coat of Dynamiq Waterbased Enamel Paint.

	Colour Range and Quantities
	· Dynamiq Waterbased Enamel Paint is available in a range of colours from our tinting system.
· Available in 1litre, 5 litres and 20 litres.

	Precautions
	· This product is not flammable.

· Contains no toxic substances and only a low level of VOC (EU regulations).

	Disclaimer
	Dynamiq cannot be held liable if the product fails due to improper surface preparation or application.
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