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PRODUCT IDENTIFICATION AND COMPANY NAME
	Product Name
	:
	Dynamiq Intelligent Coatings SuperSeal

	Product Identification
	:
	Modifying agent for: Building materials

	Supplier/Manufacturer
	:
	Dynamiq Intelligent Coatings
	
	
	

	Address
	:
	Pretoria, South Africa
	
	
	

	Website
	:
	www.dynamiq.co.za

	
	
	


1 HAZARD IDENTIFICATION
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· Inhalation at aerosol spray may damage health.

· The product hydrolyses under formation of methanol (CAS-Nr_ 57-56-1).

· Methanol is classified concerning both physical and health hazards.

· The hydrolysis rate and consequently the relevance for the hazard profile of the product is strongly dependent on the specific conditions.
2 SPECIAL HAZARDS ARISING FROM THE SUBSTANCE OR MIXTURE
· Risk of hazardous gasses or fumes in the event of fire.
· Exposure to combustion products may be a health hazard. 
· Hazardous combustion products: toxic and very toxic fumes.
3 FIRE-FIGHTING MEASURES

	Extinguishing Media
	:
	· Water mist extinguishing powder

· Alcohol-resistant foam

· Carbon dioxide

· Sand

· DO NOT use a high pressure water jet.

	Recommendations
	:
	Decomposed products are a health hazard. Use appropriate breathing apparatus. Cool closed containers exposed to fire with water to prevent ignition.



4 ACCIDENTAL RELEASE MEASURES

	Personal Precautions
	:
	· Secure the area. 

· Wear personal protection equipment. 

· Keep unprotected persons away. 

· Avoid contact with eyes and skin. 

· Do not inhale gas vapours,aerosols. 

· If material is released indicate risk. 


· Do not walk through spilled material.



	Spill
	:
	· Contain and collect spillage with absorbent material. 
· Dispose of according to local regulations. 
· Do not allow spillage to enter sewerage drains or watercourses. 


5 HANDLING AND STORAGE

	Handling
	:
	Keep container tightly closed. Keep away from heat, sparks and flame.

Eating, drinking and smoking should be prohibited in area where this material is handled, stored and processed. After handling the material, workers should wash hands and face before eating, drinking and smoking.

Always comply with health and safety regulations.

	Storage
	:
	Store in original container. Observe label precautions. Store in a cool, well-ventilated area away from incompatible materials and ignition sources.

Keep away from oxidizing agents, strong alkaline and acids.
Containers which have been opened must be carefully resealed and kept upright to prevent leakage.


6 EXPOSURE CONTROL/PERSONAL PROTECTION
	Engineering Measures
	:
	Provide adequate ventilation. Where reasonably practicable this should be achieved by the use of local exhaust ventilation and good general extraction. If these are not sufficient to maintain concentrations of particulates and solvent vapour below the OEL, suitable respiratory protection must be worn.

	Personal Protective Equipment
	:
	

	Respiration
	:
	Should ventilation be inadequate or if workers are exposed to concentrations above the exposure limit, appropriate certified respirators must be used.

	Eyes
	:
	Use safety eyewear designed to protect against splash of liquids. Never touch eyes with dirty hands or gloves.

	Ingestion
	:
	Observe the rules of hygiene. Wash hands and face before eating, drinking or smoking.

	Skin
	:
	Use protective gloves. Wash immediately in case of contact.

	Environmental Exposure Control
	:
	Do not allow product to enter sewerage drains or watercourses.



7 PHYSICAL AND CHEMICAL PROPERTIES

	Appearance
	:
	Liquid opaque colourless

	Odour
	:
	Faint

	Flash Point (ºC)
	:
	42ºC

	Boiling point
	:
	190 ºC at 1013

	Solubility
	:
	NA

	Viscosity 
	:
	(dynamic) 15- 19 mPa.s


8 STABLILTY AND REACTIVITY
	Stability
	:
	If stored and handled in accordance with standard industrial practices no hazardous reactions are known.

	Conditions to Avoid
	:
	Moisture, heat, open flames, and other sources of ignition.

	Incompatible materials
	:
	Reacts with: water. Basic substances and acids reaction causes the formation of methanol.

	Hazardous decomposition products
	:
	By hydrolysis: methanol measurements have shown the formation of small amounts of formaldehyde at temperatures above about 150 • C (302 OF) through Oxidation.


9 ENVIRONMENTAL PRECAUTIONS
· Prevent material from entering surface waters, drains or sewers arid soil. 

· Close leak if possible without risk. 

· Contain any fluid that runs out using suitable material {e.g. earth) 

· Retain contaminated water\extinguishing water. 

· Dispose of in prescribed marked [image: image2.jpg]


containers. 

· Inform authorities if substance leaks into surface waters sewerage or ground.
10 ENVIRONMENTAL HAZARDS

Not hazardous for the environment.

11 METHODS AND MATERIAL FOR CONTAINMENT AND CLEANING UP
· Take up mechanically and dispose of according to regulations. 

· Do not flush away with water. 

· For small amounts: Absorb with a neutral (non-acidic, non-basic) liquid binding material such as diatomaceous earth and dispose of according to government regulations. 

· For large amounts: Liquids may be recovered using suction devices or pumps, only air driven or properly rated electrical equipment should be used.

· Clean any slippery coating that remains using a detergent [image: image3.jpg]


soap solution or another biodegradable cleaner. 

· Silicone fluids are slippery; spills are a safety hazard. 

· Apply sand or other inert granular material to improve traction.

12 TRANSPORT INFORMATION

Not classified as dangerous for transport.
Substance does not sustain combustion.

Due to safety reasons no air transport in totes (BC) or vented packaging.

13 OTHER INFORMATION

	Date of Printing
	:
	June 2021

	Date if Issue
	:
	June 2021

	Version
	:
	1

	Notice
	:
	The information in this MSDS is based on the present state of our knowledge and on current national laws. The product is not to be used for purposes other than those specified under section 1 without first obtaining written handling instructions. It is always the responsibility of the user to take all necessary steps in order to fulfill the demand laid down in the local rules and legislation. The information in this MSDS is meant as a description of the safety requirements of our product – it is not to be considered as a guarantee of the product’s properties.
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